|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| To: | Tiburon Fire Dept  1679 Tiburon Blvd  Tiburon, Ca | | Job: | | Flag Pole Modification |
|  | |  | |  | |
| 1/5/16 | |  | | Estimate good for 30 days | |

|  |  |  |
| --- | --- | --- |
| item # | description | Cost |
| 1 | Removal of concrete flag pole sidewalk, cmu planter, driveway pavers and up to 60 yds. of dirt and remove from site. Install geo fabric and place 40 tons of baserock | 12,500.00 |
| 2 | Install # 5 – 60 grade rebar @ 12 inches each way in driveway and sidewalk area. Pour 40 yds of 3500 psi concrete | 13,800.00 |
| 3 | Fill in cmu wall at flag pole | 620.00 |
| 4 | Remove and reset flagpole | 500.00 |
| 5 | Paint flag pole while it is down | 400.00 |
| 6 | Add 2 led spot lights at flag pole on sensor | 1400.00 |
| 7 | Add drainpipe for downspout | 350.00 |
| 8 | Install 340 sq ft pavers at flagpole | 3060.00 |
|  | Total | 32,630.00 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | Total >>>>>> | $ |
|  |  |  |